**Product Overview**

|  |  |  |
| --- | --- | --- |
| **Art. no.** | **Product** | **Description** |
| 85201-10290STD | **E-307** | 6h - Immersion suit. IMO/SOLAS With bag, light & lifting strap. |
| 85201-102902XL | **E-307** |
| 82603-55290STD | **SeaEco** | 6h - Immersion suit IMO/SOLAS. With bag & lifting strap. To be worn with compatible lifejacket. |
| 82603-55290XL | **SeaEco** |
| 82606-55290MED | **SeaNordic** | 6h - Immersion suit IMO/SOLAS. With bag, light, lifting strap, sprayhood & hood with inflatable lung. To be worn w/o lifejacket. |
| 82606-55290STD | **SeaNordic** |
| 82606-55290XL | **SeaNordic** |
| 69220 | **Vacuum packing** | Vacuum packing of Immersion suits, increased service intervals from 3 to 5 years. |
| 82607-55290MED | **SeaArctic** | 6h - Immersion suit SOLAS. With bag, light, liftingstrap, sprayhood, hood with inflatable lung and NMD approved Self Righting Unit. To be worn w/o lifejacket. **Vacuum packed.** |
| 82607-55290STD | **SeaArctic** |
| 82607-55290XL | **SeaArctic** |
| 85336 | **SeaAir ( ) (4)** | 6h - **SOLAS, ETSO & NMD**-approved Offshore/integrated transportation/survival suit. To be worn w/o lifejacket. |
| 85337 | **SeaAir HUEBA ( ) (5)** | 6h - **SOLAS, ETSO & NMD**-approved Offshore/integrated transportation/survival suit - with room for compressed spare air HUEBA (excluded re-breather system). To be worn w/o lifejacket. |
| 85338 | **SeaAir Barents ( ) (6)** | **6h - SOLAS, ETSO & NMD**-approved Offshore/integrated transportation/survival suit with functional and thermal improvements. To be worn w/o lifejacket. |
| 20209 | **SeaAir Inner lining** | Inner lining for Sea Air |
| 12535 | **HPL-2** | PLB for SeaAir & SeaAir Barents 121,5 Mhz |
| 69479 | **Boot-change** | Changing to off-size boots on suits when ordering (SeaAir, E300-2, SeaWork) |
| 85458 | **HP ETSO Suit Vertical Zip** | 4h - ETSO approved passenger transportation suit. Socks. FR GoreTex Nomex fabric. Smock in neck. Socks. Loose neoprene hood in leg pocket. Gloves in sleeve pockets. To be worn with compatible lifejacket (HP ETSO Lifejacket) |
| 82968-30990STD | **HP ETSO Lifejacket ( ) ( )** | **ETSO** approved Lifejacket with 275N buoyancy. Single chamber/one automatic (UML PRO) inflation mechanism. Rebreather system with extra compressed air triggered by hydrostatic Hammar inflator. With crotch strap. |
| 20456-30590 Blue | **Lining HP ETSO Suit Vertical Zip** | Replacement lining for HP ETSO Suit. Aramide fiber-fill with Silver+ treatment. |
| **Art. no.** | **Code** | **Description** |
| 85340-30300 | **SeaWind (w/socks)** | 1h - Work/ uninsulated Immersion suit, SOLAS, LSA code 2.3 & ISO 15027-1 Class D. With lifting strap, pit zips & attached hood in back pocket. To be worn with compatible lifejacket. **GoreTex** |
| 85348-30300 | **SeaWind (w/boots)** |
| 20452-30300 | **SeaBaltic lining (Biardo)** | Fiberfill lining for SeaBaltic |
| 85134-10290 | **E 300-2** | 1h - Work/ survival suit. IMO/SOLAS LSA code 2.4 (AES). With light, lifting strap & integrated hood. May be worn w/o lifejacket. |
| 85343 | **SeaWork - Anti Exp. Suit** | 4h - Work/survival suit IMO/SOLAS LSA code 2.4 (AES) & ISO 15027-1 Class B. With light, lifting strap, integrated hood & thermal buoyancy lining. May be worn w/o lifejacket. |
| 85341 | **SeaWork - Immersion suit** | 1h - Work/uninsulated Immersion suit, IMO/SOLAS, LSA code 2.3 & ISO 15027-1 Class D. With lifting strap & integrated hood. To be worn with compatible lifejacket. |
| 20341 | **SeaWork Inner lining** | Inner lining for Sea Work, thermal protection and buoyancy |
| 85342-301403XL | **SeaRib** | 1h - Work/survival suit with integrated 150N automatic lifejacket. Approved according to NMD (>12 pass). Suit approved ISO 15027-1 Class D. Lifejacket approved according. |
| 82650-55290 | **SeaMob** | Work/survival suit, s. IMO/SOLAS LSA code 2.4 with light, lifting strap, integrated hood & inflatable lung for buoyancy. May be worn w/o lifejacket. |
| 84117-55300 | **SeaRescue** | **Rescue man suit** |
| 82690-55290 | **SeaPilot** | **Helicopter Pilot suit** |
| 84111-01290STD | **KRD Navy suit - Two models avail.** | **Quick donning suit,** 1h uninsulated Immersion suit IMO/SOLAS, LSA code 2.3 vacuum packed in belt-bag. Constructed to be worn with approved lifejacket. |
| 82791-95290STD | **NavyLife** | **Navy lifejacket** |
| 82960-01290BABY | **SeaLife** | IMO/SOLAS Passenger Lifejacket w/o light |
| 82960-01290BARN | **SeaLife** |
| 82960-01290STD | **SeaLife** |
| 82970-01290STD | **SeaLife TP** | **TP** Passenger Lifejacket with thermal protection |
| 13550 | **Safety light** | Approved safety light for suits |
| 13559 | **Safety light** | Approved safety light for lifejackets |
| 13297 | **Recharge kit UML 33g** | Cartridge black (utløsermekanisme sort), seal and CO2 Cylinder 33g |
| 13298 | **Recharge kit UML 60g** | Cartridge black (utløsermekanisme sort), seal and CO2 Cylinder 60g |
| **Art. no.** | **Code** | **Description** |
| 13294 | **CO2 Cylinder 33g** |  |
| 13364 | **CO2 Cylinder 60g** |  |
| 82940-01290BABY | **SeaPass** | Passenger immersion suit (P-2010/TPA). IMO/SOLAS LSA code 2.5 To be worn with compatible lifejacket. |
| 82940-01290JUNIOR | **SeaPass** |
| 82940-01290STD | **SeaPass** |
| 82944-05990STD | **SeaLion 150N SOLAS** | Inflatable Lifejacket IMO/SOLAS approved, double chamber w/ two automatic inflation mechanisms. With light. |
| 82945-05990STD | **SeaLion 275N SOLAS** |
| 82947-05990STD | **SeaLion 100N Junior SOLAS** |
| 82946-05990STD | **SeaLion 275N+ SOLAS** | Inflatable lifejacket IMO/SOLAS 275N Infl. Lifej. w/light, sprayhood & crotch strap (Noble) |
| 82961-05990STD | **SeaLion Leisure 150N M** | Inflatable Lifejacket ISO 12402 approved, single chamber/one **manual** (UML PRO) inflation mechanism. With crotch strap. |
| 82953-05990STD | **SeaLion Leisure 150N A** | Inflatable Lifejacket ISO 12402 approved, single chamber/one automatic inflation mechanism. With crotch strap. |
| 82965-05990STD | **SeaLion Rescue 275N** |
| 82948 | **Crotch strap** | Crotch strap **for SeaLion** life jackets, when ordered together with life jackets |
| 82950 | **Sprayhood** | Sprayhood **for SeaLion** life jackets, when ordered together with life jackets |
| 82951 | **Fire cover** | Fire retardant cover **for SeaLion** life jackets (Panotex) |
| 20171 | **SeaAir Training** | ETSO/IMO Offshore training suit wo/ inner lining and re-breeder system |
| 20172 | **Lining SeaAir Training** | Inner lining for Sea Air Training suit |
| NEW | **HP ETSO Suit Training** | Training Suit with vertical zip w/lining |
| NEW | **Lining HP ETSO Training** | Fiberfill lining for training |
| 20085 | **EBRS Re-breather** | EBRS Re-breather for Sea Air Training suit & HP ETSO Lifejacket |
| 85298 | **Training lung** | Disposable (single-use) training lung for SeaAir traing suit |
| NEW | **Training lung** | Disposable (single-use) training lung for HP ETSO Lifejacket |
| **Art. no.** | **Code** | **Description** |
| 85601 | **T P A** | Ascotherm MK I w/o sleeves |
| 85602 | **T P A** | Ascotherm MK II w/ sleeves |
| 85603 | **T P A** | Ascotherm MK IV, USCG approved |
| 85600 | **T P A** | Ascotherm Progress MK1 |
| 85344 | **SeaFish worksuit - basic** | Special work suit for the Fish farm industry without inner lining, self righting unit, gloves and hood |
| 20344 | **SeaFish Inner lining** | Inner lining for the Sea Fish work suit |
| 20054 | **Self righting unit (SeaFish)** | Self righting unit for SeaFish |
| 67004-990 | **L/S Sweater Underwear FR** | Long Sleeve Sweater 990 Black L, 50/50 Viscose/Merino wool, Flame Retardent |
| 67005-990 | **Trouser Underwear FR** | Trouser w/fly, 50/50 Viscose/Merino wool, Flame Retardent |
| 82655 | **Glove 5-F neoprene/Black** | Insulating work gloves in neoprene |
| 13384 | **Neoprene Hood** | Insulating hood in neoprene |
| 84145 | **Special suit** | Environmental wader (BS.3424-10, BS4724 part 1 and 2.) |
| 84151 | **ChemSuit** | ChemSuit, tested against a number of chemicals EN369, EN467, EN533, EN1149:1 |
| 82942 | **Polar Special** | Expedition dry suit, made to fit ski-boots. (Suit is "tailored" to the wearer) |
| 12859 | **Hanger** | White strong plastic suit hanger |
| 85405 | **Teddy Bear** | Hansen Protection Teddy Bear |